                                      Install Manual
   
       We need install the drive of the motion-card before we use the adt856-card.Otherwise,we cann't use the functions of  the motion-card.we can use the return of the function of "adt856_initial" to judge if the drive has been installed  successfully.	If the return is less than zero,the service of motion-card hasn't started-up. 

      Install Steps:

	(1)Turn off the PC and fix the card;

	(2)The system will check the new device and pop-up the dialog of "Find New Hardware Wizard" after we turn on the PC;

	(3)Choose the "Install from a list or specific location(Advanced)",then click the "Next" button;

	(4)Choose "Include this location in the search:"and cilck the "browse" button to unfold the folder of "drive";

	(5)Choose the folder of "card_drive";

	(6)Click the "Next" button to finish the installation.

   
