

(1)Under the development environment of the Borland C,  the choice "Project\Open Project"
   order create a new project;
(2)Copy the document of "ADT856H.LIB" or "ADT856L.LIB" and "adtADT856.h" to the path of new 
   project from the path of "Empolder\c or C++".
(3)Select of the "Project\Add Item"order,in the dialog between select of the  "ADT856H.LIB"
   or "ADT856L.LIB" click to the "Add" button;
(4)Add ' #include "adtADT856.h" ' to the users of the declaration procedure document;

By above-mentioned four steps,  adjust in  the functions in Dynamic-Link Library(dll). 