adt8960.h和ADT8960.lib 是单独使用ADT8960卡时使用的头文件和静态库,
调用动态链接库adt8960.dll
adt8960m.h和adt8960m.lib 是与其它类型的卡共用时使用的头文件和静态库，
调用动态链接库adt8960m.dll

VC中调用ADT8960.dll动态链接库

(1)新建一个项目；
(2)将光盘“开发包\VC”下的“adt8960.lib”和“adt8960.h”文件拷贝到新建项目的路径下；
(3)在新建项目”工作区”的”文件视图”中，右击鼠标，选择“Add Files to Project”，在插入文件  
    对话框中，文件类型选择为“Library Files(.lib)”，搜索出“adt8960.lib”并且选择，点击“OK”，
    完成静态库的加载；
(4)在源程序文件或头文件或全局头文件“StdAfx.h”的申明部分加上#include "adt8960.h"；
经过上述四步，用户即可调用动态链接库中的函数


VC中調用adt8960.dll動態鏈接庫
(1)新建一個項目；
(2)將光盤"開髮包\VC"下的"adt8960.lib"和"adt8960.h"文件拷貝到新建項目的路徑下；
(3)在新建項目"Workspace"的"FileView"中，右擊鼠標，選擇"Add Files to Project"，在插入文件的對話框
中，文件類型選擇為"Library Files(.lib)"，蒐索齣"adt8960.lib"並且選擇，點擊"OK"，完成靜態庫的加載
(4)在需要調用庫函數的源程序文件或頭文件或全侷頭文件"StdAfx.h"的申明部分加上#include "adt8960.h"
經過上述四步，用戶即可調用動態鏈接庫的函數

( 1 ) Create a new project; 
( 2 ) Copy the files of "adt8960.lib" and "adt8960.h" to the path of the new project from the path of "Empolder\vc" of CD; 
( 3 ) In "FileView" of the "Workspace", click  right mouse, then select the "Add Files to Project" command.  
      In the Dialog of "Insert Files into Project",select the file of "adt8960.lib",then click the "OK" button.
( 4 ) Add "#include "adt8960.h" to the part of the declaration of the "StdAfx.h" or the header file or the source file 
      which needs; 

By above-mentioned four steps, users can adjust in the functions in Dynamic-Link Library(dll). 