
(1)Under the development environment of the Borland C,  the choice "Project\Open Project" order 
   create a new project;
(2)Copy the document of "ADT8960H.LIB" or "ADT8960L.LIB" and "adt8960.h" to the path of new project
   from the path   of "Empolder\c or C++";
(3)Select of the "Project\Add Item"order,in the dialog between select of the  "ADT8960H.LIB" or
   "ADT8960L.LIB"  click to the "Add" button;
(4)Add ' #include "adt8960.h" ' to the users of the declaration procedure document;

By above-mentioned four steps,  adjust in  the functions in Dynamic-Link Library(dll). 